THE NATIONAL MILLING CORPORATION (SPECIFICATION FOR GRADING MAIZE STANDARDS FOR THE 1990 91 SEASON) ORDER
G.N. No. 402 of 1990
	1. This Order may be cited as the National Milling Corporation (Specification for Grading Maize Standards for the 1990/91 Season) Order.
	2. In this Order, unless the context requires otherwise–
	"broken grain" means broken maize and component parts which pass through a perforated plate sieve of aperture size 6.35mm diameter;
	"foreign matter" means any material that is not maize grain and includes other parts of the maize plant;
	"other defective grains" means maize grain which is immature, shrivelled or damaged by the action or effects of heat or excessive moisture, shrivelled or damaged by the action or effects of heat or excessive moisture such as discolouration, sprouting and mouldy; 
	"other coloured grains" means grain with pericarp of a natural colour differing from the majority of the kernels;
	"pest damaged grain" means maize grain which has been visibly damaged externally or internally, by insects or rodents.
	3. Shelled maize shall be of white varieties, of close wholesome appearance and free of commercially-objectionable odours.
	4. The test method for the shelled maize is specified in the Second Schedule to this Order.
	Notwithstanding the provisions of paragraphs 3 and 4 the grades in the First Schedule shall be used for the 1990/91 season.
FIRST SCHEDULE

	Shelled Maize
Grade I
% BY MASS	Shelled Maize
Grade I
% BY MASS	
Foreign matter	2	4	
Broken Grain	–	–	
Pest Damaged Grain	4	8	
Other Defective Grain	3	5	
Other Coloured Grain	1	2	
Moisture Content	13	13	
Live Infestation per 250g	None	None	

SECOND SCHEDULE
TEST METHOD FOR SHELLED MAIZE

	1.	Obtain representative sample from the lot and mix thoroughly. Keep material in a moisture-proof container.	
	2.	Using a moisture meter record the moisture content.	
	3.	Take 250g sub-sample. Observe condition of maize including infestation.	
	4.	Screen sub-sample over 6.35 mm diameter perforated plate sieve.	
	5.	Take weight of troughs plus hand picked foreign matter from material remaining on top of sieve. Record as foreign matter.	
	6.	From the material remaining on top of the sieve, hand pick and separate in order of priority:	
		(1)	Pest damaged grains.	
		(2)	Other defective grains.	
		(3)	Other coloured grains.	
	7.	Take individual weights of the separate materials and record as appropriate.	
	8.	Maize with component percentages greater than those shown in the grading specification and its comment shall be considered not to have achieved the grade.	

